The BL51_MCB shows a simple code banking example
with the MCB517AC prototype board.  It uses
6 memory code banks.  

To run this example enable the banking mode of
the MCB517AC board by setting the DIP switches
S1 and S2 to ON.
